=======================================================================================
                                Inventec_Horsea_BMC_V00.56.03 RELEASE NOTE
=======================================================================================
Chip    		          :  Aspeed AST2500
Version 		          :  V00.56.03
Date    		          :  2021/05/25
Checksum(SUM16)			  :  1c16
Checksum(MD5)  			  :  7f4215eaad16e545f0e228ea1aaf69e9
                             
Project Name   			  :  Horsea
Project ID     			  :  0089h
Manufacturer   			  :  Inventec Technology Corporation

1.How_To_Update.txt       - Readme first
2.BMC_Release_Note.txt    - Release Note for Notepad
rom.ima                   - 64MB BMC ROM Image File
fbmc_dos.bat              - Script file for upgrade BMC under DOS
fbmc_win.bat              - Script file for upgrade BMC under Windows
fbmc_lnx.sh               - Script file for upgrade BMC under Linux
socflash_v11800\          - Dos Flash Tool 	
winflash_v11800\          - Windows Flash Tool 	
lxflash_v11800\           - Linux Flash Tool
yafuflashWin64\           - Windows yafuflash
yafuflashLinux_x86_64\    - Linux yafuflash

Note:

Changelist V00.56.03 [05/25/2021]:
	
	Fixed Bug : 
	1. [FAE][Kuaishou_Horsea_Milan][BIOS] The SUT will hang 0xB2 in BIOS POST Screen during reboot cycle test . (60331053)
	2. [FAE][Horsea_Milan_kuaishou][BMC]Fan*_Status shows "no state defined" on the web. (60331056)
	
	Add feature : 
	1.  Add NVMe temperature to fan's airspeed strategy 

Changelist V00.55.03 [03/19/2021]:
	1. 60331004 [FAE][Kuaishou_Horsea_Milan][BMC]The BMC web interface will keep popping up error message after logging in to the web with a user with user privileges
	2. 60331018 [FAE][Kuaishou_Horsea_Milan][BMC]No found any info about CPU/DIMM/PCIE device in BMC WEB.
	3. 60331028 [FAE][Kuaishou_Horsea_Rome][BMC]The other FAN(s) speed can't increase after remove one FAN device.
	4. 60331029 [FAE][Kuaishou_Horsea_Rome][BMC]Failed to check Liteon PSU FW version by the OEM command after update FW completely
	5. 60331030 [FAE][Kuaishou_Horsea_Milan][BMC] BMC sdr elist about DIMM is not displayed in order 
	6. 60331034 [FAE][Kuaishou_Horsea_Milan][BIOS] The BIOS version is not displayed correctly in the WebUI.

Changelist V00.54.03 [03/03/2021]:
	1. (fixed) 60331017 Found sel error if using Chicony PSU(R800AV07P,FW:01.01.01) as Power source on platform of kuaishou SUT
	2. (fixed) 60331012 Change the name of the DIMM to be consistent with the screen printing on the motherboard
	3. (fixed) Add title of login interface	
	4. (fixed) 60331005 The "Most recent Addition" shows "02/07/2106 06:28:15" in ipmitool sdr info.
	5. (fixed) 60331014 No found BMC boot up Sel log in sel list after BMC reset completed
	6. (fixed) 60331022 Fail to disable the power button by the command "ipmitool raw 0x00 0x0A 0x01"

Changelist V00.53.03 [02/04/2021]:
	1. Modify Sensor name PSU_Power_In to PSU_Power
	2. Fixed the problem of printing SDR list too long
	3. Fix that the BMC special port IP cannot be obtained

Changelist V00.52.03 [01/16/2021]:
	1.Modify Sensor name PSU_Pin to PSU_Power_In
        2.Disable NCSI ShareLink Mmodel
        3.Enable DCMI feature.
        4.Modify the power on Strategy of BMC
        5.ipmitool get BIOS version
                  ➜  Horsea_kuaishou sudo ipmitool -H 10.99.104.29 -U admin -P kuaishou raw 0x2e 0x03 0xa9 0x19 0x00 0x06 0x00
 	                  a9 19 00 48 4f 52 53 53 30 35 30
                  ➜  Horsea_kuaishou



Changelist V00.51.03 [12/25/2020]:
	1.Delete sensor DiskG_temp.
	2.Delete sensor Card0_temp.
	3.Delete sensor Card1_temp.
	4.Adjust the order of sensors.
	5.Turn off sharelink mode
	6.Modify srnsor name. 
	7.Enable WEB SOL

Changelist V00.50.03 [12/20/2020]:
	1.Complete the customized requirements of customers.
	2.Modify the CPU's setpoint to Tjmax - 20. 
	3.Modify Product ID to 0x89.

	
