; How to update BMC firmware 
;================================================================
1.Usage Description:
- For DOS Execution Environment Use Script: fbmc_dos.bat
- For Windows Execution Environment Use Script: fbmc_win.bat
- For Linux Execution Environment Use Script: ./fbmc_lnx.sh

2.File List and MD5:
- BMC firmware Image: rom.ima  
	MD5 : e2ffc21b3119d59067abab6fe31a4d1f

- Dos Flash Tool: socflash_v11800\socflash.exe 	
	MD5 : 21cf9497d9aa80c73d08ca6494877c0d
	
- Windows Flash Tool: winflash_v11800\socflash.exe 	
	MD5 : 6644d8b949365cb41e4bb77c40305c3d
	
- Windows Flash Tool(64Bit): winflash_v11800\socflash_x64.exe 	
	MD5 : f9fa860c1531df938ae92234234fbe96 
	
- Linux Flash Tool: ./lxflash_v11800/socflash 
	MD5 : e42472f6cb7d5f09ad8240e1ce237dce 
	
- Linux Flash Tool(64Bit): ./lxflash_v11800/socflash_x64
	MD5 : 19401831a204ee498e84c2dcb9c0550e 

3.Socflash Version - V1.18.00
	E.G.
  .\socflash.exe if=<BMC.ima>
  .\socflash_x64.exe if=<BMC.ima>
  ./socflash if=<BMC.ima>
  ./socflash_x64 if=<BMC.ima>
